**Modified wooden drum (M2)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Variable** | **# strikes** |  | **Mean (%)** |  |
|  |  | **Single** | **Double** | **Misses** |
| ***Seed size*** | **N** |  |  |  |
| 2585 | 200 | 78.4 | 2.6 | 18.3 |
| 3968 | 200 | 35.0 | 59.0 | 6.0 |
| **Mean** | 400 | 56.2 | 31.5 | 12.3 |

**Note;**

1. Strikes without misses constituted 81.1 and 94.0% using 2,585 and 3968 seed sizes respectively
2. The misses were attributed mainly to bridging of the gap between drum cavity and wall of interior housing with seeds
3. Overall and irrespective of the seed size, strikes accompanied with the delivery of seeds constituted 87.7% of the total strikes
4. The drum cavity was drilled by Robert and as such he may need to give us the tips he used to achieve fairly decent results compared to the previous drums we modified